,ControlsControllerType##OTHER##,DimensionsOverallWidth##OTHER##,ExtractAirOperation##OTHER##,SashOperation##OTHER##,BIMObjectName##OTHER##,NBSVariantId##OTHER##,IsStandard##OTHER##,Width##LENGTH##MILLIMETERS,ModelNumber##OTHER##,Name##OTHER##,NominalHeight##LENGTH##MILLIMETERS,NominalLength##LENGTH##MILLIMETERS,NominalWidth##LENGTH##MILLIMETERS,Size##OTHER##
PPFC150–ProModelVariableAirVolume,"Touch screen control panel, 9-inch",1500 mm,Facility to vary extract volume flow rate,"Powered, automatic",NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC150–ProModelVariableAirVolume,9ac2d778-2654-e1f4-8540-b9c6b08c0626,0,1500,PPFC150,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC150–ProModelVariableAirVolume_TionGlobalLtd,2320,1500,830,1500 x 830 x 2320 mm
Bespoke–ProModelVariableAirVolume,"Touch screen control panel, 9-inch",Bespoke,Facility to vary extract volume flow rate,"Powered, automatic",NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_Bespoke–ProModelVariableAirVolume,2615a157-d804-7311-97d3-5f7dd04cebf5,0,1200,n/a,General-purposeFumeCupboards_DuctedFumeCupboard_Bespoke–ProModelVariableAirVolume_TionGlobalLtd,0,0,0,Bespoke
PPFC180–StandardModelConstantAirVolume,"Touch screen control panel, 7-inch",1800 mm,Continuous,Manual,NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC180–StandardModelConstantAirVolume,ce89561c-5fd1-27a9-443b-c08b1e0d825f,1,1800,PPFC180,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC180–StandardModelConstantAirVolume_TionGlobalLtd,2320,1800,830,1800 x 830 x 2320 mm
PPFC120–ProModelVariableAirVolume,"Touch screen control panel, 9-inch",1200 mm,Facility to vary extract volume flow rate,"Powered, automatic",NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC120–ProModelVariableAirVolume,53a69f7e-3111-6f32-1624-ec70caad3dcc,0,1200,PPFC120,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC120–ProModelVariableAirVolume_TionGlobalLtd,2320,1200,830,1200 x 830 x 2320 mm
Bespoke–StandardModelConstantAirVolume,"Touch screen control panel, 7-inch",Bespoke,Continuous,Manual,NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_Bespoke–StandardModelConstantAirVolume,153d4123-64d8-3364-6d45-bf14785c7afd,1,1200,n/a,General-purposeFumeCupboards_DuctedFumeCupboard_Bespoke–StandardModelConstantAirVolume_TionGlobalLtd,0,0,0,Bespoke
PPFC2000–ProModelVariableAirVolume,"Touch screen control panel, 9-inch",2000 mm,Facility to vary extract volume flow rate,"Powered, automatic",NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC2000–ProModelVariableAirVolume,14678465-1378-297e-b871-369c2de5f5ba,0,2000,PPFC2000,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC2000–ProModelVariableAirVolume_TionGlobalLtd,2320,2000,830,2000 x 830 x 2320 mm
PPFC120–StandardModelConstantAirVolume,"Touch screen control panel, 7-inch",1200 mm,Continuous,Manual,NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC120–StandardModelConstantAirVolume,e55b91e4-4e02-72d4-e912-1736a8e9cb07,1,1200,PPFC120,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC120–StandardModelConstantAirVolume_TionGlobalLtd,2320,1200,830,1200 x 830 x 2320 mm
PPFC2500–StandardModelConstantAirVolume,"Touch screen control panel, 7-inch",2500 mm,Continuous,Manual,NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC2500–StandardModelConstantAirVolume,e035c0a3-f32a-6e3f-9dec-4a216273fe28,1,2500,PPFC2500,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC2500–StandardModelConstantAirVolume_TionGlobalLtd,2320,2500,830,2500 x 830 x 2320 mm
PPFC2500–ProModelVariableAirVolume,"Touch screen control panel, 9-inch",2500 mm,Facility to vary extract volume flow rate,"Powered, automatic",NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC2500–ProModelVariableAirVolume,137334fc-2787-716a-aee6-0fd7601206a7,0,2500,PPFC2500,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC2500–ProModelVariableAirVolume_TionGlobalLtd,2320,2500,830,2500 x 830 x 2320 mm
PPFC180–ProModelVariableAirVolume,"Touch screen control panel, 9-inch",1800 mm,Facility to vary extract volume flow rate,"Powered, automatic",NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC180–ProModelVariableAirVolume,606f0c0e-8f8d-cf97-6bf7-5a1b8cc0f037,0,1800,PPFC180,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC180–ProModelVariableAirVolume_TionGlobalLtd,2320,1800,830,1800 x 830 x 2320 mm
PPFC150–StandardModelConstantAirVolume,"Touch screen control panel, 7-inch",1500 mm,Continuous,Manual,NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC150–StandardModelConstantAirVolume,4ed70f01-1e44-a37c-a2a9-7ed9c0cc0428,1,1500,PPFC150,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC150–StandardModelConstantAirVolume_TionGlobalLtd,2320,1500,830,1500 x 830 x 2320 mm
PPFC2000–StandardModelConstantAirVolume,"Touch screen control panel, 7-inch",2000 mm,Continuous,Manual,NBS_TionGlobalLtd_General-purposeFumeCupboards_DuctedFumeCupboard_PPFC2000–StandardModelConstantAirVolume,b0184674-1c13-5cdb-f811-2b08aebdad64,1,2000,PPFC2000,General-purposeFumeCupboards_DuctedFumeCupboard_PPFC2000–StandardModelConstantAirVolume_TionGlobalLtd,2320,2000,830,2000 x 830 x 2320 mm
